Dropped Kerb/Hard standing

Specification

Name:
Address:
Tel:

Overall Aim Of Scheme

To provide access to and from the dwelling and adequate parking facilities for a disabled person with / without carer assistance.

Specifications

Create dropped kerb facilities to front / rear / side access of property.

Create vehicle hard standing to front / rear / side access of property.

Special Features

Hard standing area required for ambulant disabled person should be approx. 3000mm x 4800mm.

Hard standing area required for wheelchair dependent person to be approx. 3600mm x 4800mm.

Other Requirements

General

The design and layout of the above brief must be agreed with the Occupational Therapist before final arrangements are made for the manufacture or installation.

Occupational Therapist:
Assistant Team Manager:
Date:

Swindon Borough Council Occupational Therapy Service – Specification

Dropped Kerb / Hard Standing

Page 1 of 2

SPECIFICATIONS OF SCHEME

ECC Social Services

2002-01-14

Swindon Borough Council

Marion Wilson