Exterior Steps and Half Steps

Specifications

Name:
Address:
Tel:

Overall Aim of Scheme

To adapt / adapt and construct / construct concrete step / steps at the front door / at the side door / at the back door / to give access along a path / to give access to necessary facilities.

Specifications

Surface to be of roughened slip resistant finish.

Each step to have a tread of _____mm

Each step to have a riser height of _____mm

Each step to be a minimum width of _____mm

Completed steps to be uniform in height and depth.

Alter the dimensions of the original step to match the above

Supply single / double vertical grabrail(s) adjacent to the door frame on the right / left / both side(s). To be sited with lowest end _____mm high above finished ground level.

OR

Supply single / double horizontal grabrail(s) on the left / right / both side(s). To extend 300mm beyond the top / bottom step x _____mm high

Special features

Steps to be formed in conjunction with associated ramp specification

Widen path to a minimum of _____mm.

Occupational Therapist:
Assistant Team Manager:
Date:

Swindon Borough Council Occupational Therapy Service – Specification

Exterior Steps and Half Steps

Page 2 of 2

Exterior Steps and Half Steps

Diana Coombs

2002-01-14

Swindon Borough Council

Home