New Toilet Facility

Specifications

Name:
Address:
Tel:

Overall aim of Scheme

To provide an extension / conversion to the ground / first floor of the property to create an area with toilet and basin.

Specifications

Walls to be constructed / strengthened to take wall mounted grab rails.

Ceiling joists to be constructed / strengthened to take ceiling track hoist.

Room size to be approx.:	1900mm x 900mm / 1900mm x 1500mm / 2000mm x 2100mm

Supply and install toilet (not close coupled) with seat height from finished floor level:

400mm – 450mm / 450mm – 500mm

_____mm (using a plinth).

Fit with standard / spatulate flush handle on left / right side of the toilet (facing).

Waste pipe to be directed straight out of the back of the toilet.

Allow 200 / 300mm space on wall side of the toilet.

Allow 950mm space from the centre of the toilet to the adjacent wall on left / right side (facing) for sideways transfers.

Supply and install pedestal / bracket mounted wash hand basin at height of _____mm from finished floor level, with knee clearance below bowl not less than 600mm.

Fit with long / short quarter turn lever taps.

Provide access via an inward hinged / outward hinged / sliding / folding door to give a clear opening of 720 / 840 / 900mm.

Install _____ x _____mm horizontal / vertical / angled rails beside the toilet. Exact position to be agreed on site with the Occupational Therapist.

Install _____ drop down rail(s) to the right / left / both side(s) of the toilet. Exact position to be agreed with the Occupational Therapist.

Supply suitable form of ventilation eg:

Occupational Therapist:
Assistant Team Manager:
Date:

Swindon Borough Council Occupational Therapy Service – Specification

New Toilet Facility

Page 2 of 2

New Toilet Facility

Diana Coombs

2002-01-14

Swindon Borough Council

Swindon Borough Council