Specialist Toilet Facility

Specifications

Name:
Address:
Tel:

Overall Aim of Scheme

To provide a specialist toilet to enable the disabled person to manage their personal hygiene with / without carer assistance.

Specifications

Supply and install specialist toilet.

Supply and install thermostatically controlled flush and warm water wash. NB hot water supply not to exceed 38 degrees Centigrade.

Supply and install warm air dryer.

Supply and install conventional flush.

Supply and install standard elbow pads for flushing.

Special Features

Supply and install hand switch.

Supply and install foot switch to be floor/wall mounted.

Supply and install special fingertip pressure switch for light touch.

Supply and install infrared control

Supply and install raised shaped plinth to achieve a total height of approx. mm. from finished floor level.

Supply and install extended douche arm with single/twin spray.

Supply and install back bar.

Supply and install upholstered soft seat.

Install unit approx. mm forward of wall and box in behind.

Seat switch to be by-passed to allow for foot/hand switch operation.

Pressure sensor on seat to be by-passed for use with over toilet chair

Supply and install X mm horizontal/vertical/angled/drop down grab rails at side of WC unit (position to be agreed on site with Occupational Therapist).

Supply slip resistant flooring to the whole floor area.

Other Requirements

.

Occupational Therapist:
Assistant Team Manager:
Date:

Swindon Borough Council Occupational Therapy Service – Specification

Specialist Toilet Facility

Page 2 of 2

SPECIFICATIONS OF SCHEME

ECC Social Services

2002-01-14

Swindon Borough Council

Marion Wilson