Specialist Bath

Specifications

Name:
Address:
Tel:

Overall Aim of Scheme

To provide a specialist bath to enable the disabled person to manage their personal hygiene with / without carer assistance.

Specifications

Remove the existing bath.

Supply and install a specialist bath, e.g: _____

Size approx. _____mm X _____mm.

Supply and install integral bath seat.

Supply and install armrests that can be individually raised.

Supply and install recessed handgrips.

Supply and install air switch handset.

Supply and install seat locking release lever.

Supply and install pop-up waste.

Supply and install tiling to prevent water damage.

Special Features

Bath seat to lower below the outside edge of the bath and be able to rotate through 180(.

Supply and install slip-resistant floor covering to whole floor area.

Supply and install an appropriate form of ventilation.

Supply and install an appropriate form of heating.

Supply and install/Widen internal doorsets to give a minimum clear opening of 712mm / 788mm / 865mm /……..mm.

Supply and install sliding door to bathroom.

Re-hang bathroom door to opposite jamb.

Supply and install quarter turn short/long lever taps to bath.

Supply slip resistant flooring to the whole bathroom area.

Other Requirements

The design and layout of the above brief must be agreed with the Occupational Therapist before final arrangements are made for the manufacture or installation

Occupational Therapist:
Assistant Team Manager:
Date:

Swindon Borough Council Occupational Therapy Service – Specification

Specialist Bath

Page 2 of 2

SPECIFICATIONS OF SCHEME

ECC Social Services

2002-01-14

Swindon Borough Council

Marion Wilson