Steplift

specifications

Name:
Address:
Tel:

Overall Aim of Scheme

To provide steplift to front / rear / side / interior of property to enable the disabled person to access internal / external facilities

Lift to accommodate wheelchair / ambulant user with / without attendant

Weight of service user:	_____

Specifications

Supply and install internal / external steplift to lift over the front / rear / side / internal steps.

Manufacturer	Model	External dimensions	Internal dimensions
____mm x ____mm	____mm x ____mm
____mm x ____mm	____mm x ____mm

Supply and install wall mounted push button controls at height _____mm.

Supply and install push button controls with within the lift positioned left / right hand side of unit.

Supply and install built-in ramp for wheelchair access.

Supply and install dedicated power supply.

Supply and install pressure sensitive surfaces to the lift.

Supply and install slip-resistant surface to platform and ramp.

Special Features

Supply and install manual emergency lowering device.

Supply and install safety key switch to immobilise the lift.

Supply and install integral bridging plate.

Supply and install interlocked safety gate.

Supply and install exterior light.

Supply and install alarm system.

Supply and install wander lead control.

Create level access threshold between platform and inside of property for wheelchair mobility.

Supply and install external doorset with minimum clear opening of 900mm.

Construct concrete base and path in preparation for step lift installation.

Other Requirements

Occupational Therapist:
Assistant Team Manager:
Date:

Swindon Borough Council Occupational Therapy Service – Specification

Steplift

Page 2 of 2

Bed/Bathroom Extenstion

Diana Coombs

2002-01-14

Swindon Borough Council

Swindon Borough Council