Through Floor-Lift

specifications

Name:
Address:
Tel:

Overall Aim Of Scheme

To provide a through-floor lift between floors to enable access to all essential facilities with / without carer assistance.

Specifications

Make necessary associated structural preparations.

Supply and install a wheelchair / compact through floor lift, i.e:

Manufacturer	Model	External dimensions	Internal dimensions
____mm x ____mm	____mm x ____mm
____mm x ____mm	____mm x ____mm

Height of service user	Weight of service user

Supply and install power operated controls with push buttons within the lift, positioned left / right hand side facing carriage, at height _____mm.

Supply and install wall mounted power operated controls with push buttons on both floor levels.

Supply and install safety key switch to immobilise the lift.

Supply and install dedicated power supply.

Supply and install pressure sensitive surfaces to the carriage.

Supply and install interior light.

Special Features

Supply and install a fully enclosed shaft for the lift on the outside/inside of the property.

Supply and install fixed/folding/sliding seat at height approx. mm. from finished floor level.

Supply and install a fully/partially enclosed carriage for the lift.

Supply and install alarm system.

Supply and install telephone hand set, fitted to the lift carriage positioned left/right hand side of carriage.

Supply and install built in ramp for wheelchair access.

Supply and automatic door opener

Supply remote control switches inside/outside the lift

Supply joystick controls inside/outside the lift

Other Requirements

The design and layout of the above brief must be agreed with the Occupational Therapist before final arrangements are made for the manufacture or installation.

Occupational Therapist:
Assistant Team Manager:
Date:

Swindon Borough Council Occupational Therapy Service – Specification

Through Floor-Lift

Page 3 of 3

Bed/Bathroom Extenstion

Diana Coombs

2002-01-14

Swindon Borough Council

Swindon Borough Council